
/////////////////////////////////////////////////////////////////////////////////////

       SII RP JavaPOS Driver


                                              Seiko Instruments Inc.
/////////////////////////////////////////////////////////////////////////////////////

=====================================================================================
  BEFORE USING THE SOFTWARE
=====================================================================================
Read the SOFTWARE LICENSE AGREEMENT (LICENSE_EN.txt).

When all or part of this software is installed to computer, or this software is used,
you are deemed to accept SOFTWARE LICENSE AGREEMENT.

=====================================================================================
  TARGET DEVICE
=====================================================================================
   > RP-E10 Series
   > RP-D10 Series

=====================================================================================
  INTRODUCTION
=====================================================================================
Seiko Instruments Inc. provides software;
    > SII RP JavaPOS Driver Ver.1.11 ( May,2026 )

=====================================================================================
  FOLDER STRUCTURE
=====================================================================================
JavaPOS
│  JavaPosUtility.bat               //Batch file for launching the configuration program
│  jpos.xml                         //"Java POS Entry Registry" configuration file
│  logo.bmp                         //Logo file for sample application
│  SampleApp.bat                    //Batch file for launching sample application
│
├─lib
│          JavaPosUtility.jar        //Configuration program
│          jpos1135-controls.jar     //Device control
│          SampleApp.jar             //Sample application
│          siijpos.CashDrawer.RP.jar //CashDrawer device service
│          siijpos.comm.jar          //Communication library
│          siijpos.POSPrinter.RP.jar //POSPrinter device service
│          *.jar                     //Other libraries
│
└─Samples
    └─SiiJavaPOSDriver_Samples
        └─*.*                       //Sample source code

=====================================================================================
  SYSTEM REQUIREMENTS
=====================================================================================
 [[ Supported operating system ]]
   > Microsoft Windows 10  (32bit/64bit)
   > Microsoft Windows 10 IoT Enterprise  (32bit/64bit)
   > SUSE Linux Enterprise 11 (32bit/64bit)

 [[ Java]]
   > Java SE 6 6u45 or later
  * 64-bit Java support is Java SE 8 or later

 [[ Printer Driver]]
   > For RP-D10: RP-D10 series printer driver
   > For RP-E10: RP-E10 series printer driver
　* Windows Only,The driver name must include the printer model name "SII RP-x10"

=====================================================================================
  VERSION HISTORY
=====================================================================================
　 > Ver.1.20
    ・Changed to support Linux only

   > Ver.1.11
    ・Fixed a bug that invalidated the digital signature.

   > Ver.1.10
    ・Supports Windows 10, Supports the latest Java.
    ・Fixed a bug that no error occurs even if page mode is specified during 180 degree rotation printing.
    ・Fixed a bug that no error occurs even if PowerNotify is set after Eanble.
    ・Fixed a bug that an error occurs when 0 is specified for the cutPaper parameter.
    ・Fixed a bug that returns an error when calling DeviceEnabled up to claim.
    ・Fixed a bug that FlagWhenIdle is not reset even if it recovers from an error during asynchronous output.
    ・Fixed a bug that validateData judgment succeeds even though it is an invalid escape sequence.
    ・Fixed a bug that the image alignment position does not match the specified position in the case of rotation printing.
    ・Fixed a bug that Disable processing succeeds when state error (4) due to FreezeEvent (True) occurs.
    ・Fixed a bug that the print position is incorrect when printing repeatedly in page mode.
    ・Added improvement processing such as initializing the printer at open.
    ・Fixed a bug that the magnification of escape sequence cannot be set individually in one line of PrintNormal transmission.
    ・Fixed a bug that the print position of the image was incorrect during Left-right rotation printing by ESC|B or printBitmap.
    ・Added improvement processing so that horizontal position correction is effective for printing of setBitmap in page mode.
    ・Fixed a bug that Japanese printer driver name is not recognized.
    ・Other minor corrections.


   > Ver.1.00
	Release
 
=====================================================================================
Seiko Instruments Inc.
Web: http://www.sii.co.jp/sps/eg/
 
Copyright(C) 2019-2026 Seiko Instruments Inc.
The information contained herein shall not be reproduced in whole or in part without the prior written approval of SII.
SII reserves the right to make changes without notice the specifications and materials contained herein.
SII is not liable for any damages, losses, caused by or relating to the use of this product, nor for any expenses incurred for defraying such.
SII is a trademark of Seiko Instruments Inc.
Other application software mentioned herein may be trademarks and/or registered trademarks of their respective companies.
